{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["报价单","附件","Sheet3"],"not_rendered":{"images":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"报价单","index":0,"n_rows":23,"n_cols":13,"rows_kept":23,"merged":[[0,0,0,12],[1,10,1,12],[2,0,2,12],[3,0,3,12],[4,2,4,3],[8,2,8,3],[9,1,9,5],[9,6,9,12],[10,0,13,0],[10,1,10,2],[10,3,10,12],[11,1,11,2],[11,3,11,12],[12,1,12,2],[12,3,12,12],[13,1,13,2],[13,3,13,12],[14,0,19,6],[14,7,19,12],[20,1,20,12],[21,1,21,12],[22,1,22,12]],"flags":["formulas_cached_only"]}
["非苗采购报价单（供应商填写）"]
[{"$nulls":10},"表格编码：DQST-ZC-006"]
["项目名称：泰和县马市生态文化特色小镇PPP项目                                                 项目编号：2017019"]
["供方：                                联系人：                   联系方式：                      报价日期："]
["序号","品种名称","规格型号",null,"质量等级","品牌","单位","数量","含税单价（元）","合价（元）","货源地","税率","备注"]
[1,"灯具","单臂灯","6m高\n1、详细参数见附表",null,null,"套",398,{"$nulls":3},{"v":0.13,"d":"13%"},"60w灯具"]
[2,"灯具","双臂灯","6m高\n1、详细参数见附表",null,null,"套",56,{"$nulls":3},{"v":0.13,"d":"13%"},"2盏60w灯具"]
[3,"灯具","单臂灯","9m高（入口大桥）\n1、详细参数见附表",null,null,"套",10,{"$nulls":3},{"v":0.13,"d":"13%"},"130w灯具"]
[]
["总计","小写：",{"$nulls":4},"大写："]
["备注","1、付款方式",null,"A）合同签订后 5 日内，支付至合同价款的 20 %作为预付款；\nB）货物运至指定地点，经验收合格后支付至已供货物价款的 60 %；\nC) 灯具安装完工调试合格且试运行一个月经验收合格支付至已供货物款的 80 %；\nD) 已供货物价款的 20 %在需方验收合格之日起一年后一次性无息支付。\nE)付款方式：电汇、转账、承兑等"]
[null,"2、交货地点",null,"吉安市泰和县马市镇蜀口洲环岛路、服务中心"]
[null,"3、供方承诺",null,"以上报价真实有效，实际到货以项目现场验收为准"]
[null,"4、其他"]
["供方签字：",{"$nulls":6},"供方盖章："]
[]
[]
[]
[]
[]
["备注：","1、此表为非苗采购比价单附件，比价单上传需附供方签字盖章报价单（无效报价单不计入有效询价单位）；"]
[null,"2、报价需附相应材料小样（无法提供小样附实景参数照片）。如遇报价照片与实际到货照片不符，需方有权退货并追究其责任。"]
[null,"3、材料价为到项目工地全费用价，工地全费用价含材料原价、材料运杂费、运输损耗费、采购及保管费（验收前）、供应商利润、增值税发票等。"]

{"sheet":"附件","index":1,"n_rows":27,"n_cols":5,"rows_kept":27,"hidden":true,"merged":[[0,0,0,3],[1,2,1,3],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[10,2,10,3],[11,2,11,3],[12,2,12,3],[13,2,13,3],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[18,2,18,3],[19,2,19,3],[20,0,20,4],[22,0,22,3],[24,4,26,4]],"flags":["formulas_cached_only"]}
["附件                                 路灯参数"]
["序号","型号","单晶",null,"单晶"]
[1,"光伏板功率","60W",null,"130W"]
[2,"光通量(单颗）",">10 lm ",null,">10 lm "]
[3,"LED芯片","台湾晶元（或同档次）",null,"台湾晶元"]
[4,"CTC微光发电板(弱光测试）",{"v":0.1988,"d":"19.88%"},null,{"v":0.1988,"d":"19.88%"}]
[5,"CTC微光发电板(强光测试）","24-25%",null,"24-25%"]
[6,"电压","12V",null,"24V"]
[7,"锂电池","30Ah",null,"40Ah"]
[8,"色温","3000K-9000K",null,"3000K-9000K"]
[9,"显色指数","75-85",null,"75-85"]
[10,"每天照明时间","12-15h",null,"12-15h"]
[11,"抗阴雨天数","365天",null,"365天"]
[12,"使用环境","﹣40℃-70℃",null,"﹣40℃-70℃"]
[13,"灯具材质","全铝合金",null,"全铝合金"]
[14,"锂电池寿命","3-5年",null,"3-5年"]
[15,"光源寿命","＞80000小时",null,"＞80000小时"]
[16,"控制器防护等级","IP67",null,"IP67"]
[17,"整灯防护等级","IP65",null,"IP65"]
[18,"灯柱规格","高度6米，上下口径60*140mm,壁厚3mm，出臂1米，直径60，厚2.5，法兰260*260*12mm，灯杆材质为热镀锌钢管 ",null,"高度9米，灯杆臂厚4mm，上150*150mm，下200*200mm，法兰400*400mm，出臂1.2m，灯杆材质为热镀锌钢管"]
["1.产品价格为到最终用户指定现场价格(含运保费)，应包含从安装验收合格后起24个月的保修期费用、不含税。"]
[]
["灯具图样确认表"]
["序号","类型","单价","图片","备注"]
[1,"单臂6m高","灯杆为圆管",null,"灯杆样式为统一样式，双臂为意向效果图，实际使用参照单臂样式"]
[2,"双臂6m高","灯杆为圆管"]
[3,"单臂9m高","灯杆为方管"]

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}